GRIFCO Model ML5102SBF (L/R), eDrive +2.0 Operator for Spring Balanced Roller Shutters up to 36m² in size. Supplied with a 1.0Hp 1Ph 0.75kW (6.00A) Motor and Purpose-designed Gearbox for Low Cycle (10% run time) applications. Complete with Absolute Positioning Encoder (APE), Smoke Baffle Functionality (SBF) and Automatic Chain-Engage Mechanisim (ACEM). Rated IP44 and Certified to AS/NZS 60335.2.103. Compatible with Optional Controller Upgrade Model C23B - eDrive +2.0 Advanced Wall Control with Key Switch and Mounting Plate Kit Model SK1018 (inc. Mounting Plate, 10B Sprocket, Drive Chain and 8m Hauling chain). Made in Australia.