GRIFCO Model ML5103 (L/R), eDrive +2.0 Operator for Spring Balanced Roller Shutters up to 36m² in size. Supplied with a 1.0Hp 3ph 0.75kW (2.30A) Motor and Purpose-designed Gearbox for Low Cycle (10% run time) applications. Complete with Absolute Positioning Encoder (APE) and Automatic Chain-Engage Mechanisim (ACEM). Rated IP44 and Certified to AS/NZS 60335.2.103. Compatible with Optional Controller Upgrade Model EB1 - eDrive +2.0 Expansion Board with High Lid and Mounting Plate Kit Model SK1018 (inc. Mounting Plate, 10B Sprocket, Drive Chain and 8m Hauling chain). Made in Australia.