GRIFCO Model 58017FFH (L/R), Fire Shutter Operator for Spring Balanced Roller Shutters up to 36m² in size. Supplied with a 1.5Hp 3ph 1.10kW (2.55A) Motor and Purpose-designed Gearbox for Low Cycle (10% run time) applications. Complete with Mechanical Limit System, Fusible Link (fuses at 71°C), Holding Magnet and Automatic Chain-Engage Mechanism (ACEM). Rated IP44 and Certified to AS/NZS 60335.2.103. Compatible with Optional Controller Upgrade Model GLMe2 - eDrive +2.0 Logic Upgrade with Key Switch and Mounting Plate Model MP001. Made in Australia.