GRIFCO Model 58019FF (L/R), Fire Shutter Operator for Spring Balanced Roller Shutters up to 28m² in size. Supplied with a 1.0Hp 3ph 0.75kW (2.30A) Motor and Purpose-designed Gearbox for Low Cycle (10% run time) applications. Complete with Mechanical Limit System, Fusible Link (fuses at 71°C), Flameproof (EXD) Certification and Automatic Chain-Engage Mechanism (ACEM). Rated IP44 and Certified to AS/NZS 60335.2.103. Compatible with Optional Controller Upgrade Model RG374-LB3E007-EX - Reversing Starter for basic Up / Stop / Down Control, Dust Ignition Proof and Mounting Plate Model MP001. Made in Australia.