GRIFCO Model GSDK-R2.4M-GLCPSRK, S-Drive Commercial Door Operator for Spring Balanced Sectional Doors up to 26m² in size, 315.5kg in weight and 2.4m in height. Continuous (100% run time) Duty Cycle with a door speed of 20cm/sec. Supplied with a 24V DC 230-240 VAC 50Hz, 400W Motor and Purpose-design Gearbox. Supplied with Integral Battery Back Up for Operation in the Event of a Power Failure, GLCPS Monitored Light Curtain and 2 x E960G Transmitters. Compatible with Optional Upgrade STAR1000EVO and GTM-E960G-50 Transmitter Management Device and 50 x E960G Transmitters.