GRIFCO Model HDHWFFH (L/R), Fire Shutter Manual Hoist for Spring Balanced Roller Shutters up to 16m² in size. Complete with Fusible Link (fuses at 71°C) and Holding Magnet. Suitable for Mounting Plate Model MP005 and Galvanised Long Link 5mm Hand Chain – 8m length Model HC5MM8. Made in Australia.