GRIFCO Model MH102M (L/R), mDrive Operator for Spring Balanced Roller Shutters up to 30m² in size. Supplied with a 1.0Hp 1Ph 0.75kW (4.35A) Motor and Purpose-designed Gearbox for High Cycle (30% run time) applications. Complete with Mechanical Limit System and Automatic Chain-Engage Mechanisim (ACEM). Rated IP44 and Certified to AS/NZS 60335.2.103. Compatible with Optional Controller Upgrade Model RG376-LB3E009 - Reversing Starter for basic Up / Stop / Down Control and Mounting Plate Kit Model SK1018 (inc. Mounting Plate, 10B Sprocket, Drive Chain and 8m Hauling chain). Made in Australia.