GRIFCO Model MH103MD (L/R), mDrive Operator for Spring Balanced Roller Shutters up to 36m² in size. Supplied with a 1.0Hp 3ph 0.75kW (1.95A) Motor and Purpose-designed Gearbox for High Cycle (30% run time) applications. Complete with Mechanical Limit System, Dust Ignition Proof Certification and Automatic Chain-Engage Mechanism (ACEM). Rated IP66 and Certified to AS/NZS 60335.2.103. Compatible with Optional Controller Upgrade Model RG374-LB3E007-EX - Reversing Starter, Up / Stop / Down Control, Dust Ignition Proof and Mounting Plate Kit Model SK1018 (inc. Mounting Plate, 10B Sprocket, Drive Chain and 8m Hauling chain). Made in Australia.