GRIFCO Model GLD-RDO, LR-Drive Commercial Door Operator for Spring Balanced Roller Doors up to 28m² in size, 270kg in weight and 5.5m in height. 50 cycles/day Duty Cycle with a door speed of 21 seconds to open a 2.4m high door. Supplied with a 24V DC 230-240 VAC 50Hz, 150W Motor and Purpose-design Gearbox. Supplied with detachable Battery Backup, E138G Wireless Wall Control and 2 x E960G 4-Channel Keyring Transmitters. Compatible with GWS series of flashing lights and sounders, key activation key switches and Grifco Transmitter Management.