GRIFCO Model GLD-SDO-R3.0M, LS-Drive Commercial Door Operator for Spring Balanced Sectional Doors up to 15m² in size, 160kg in weight and 3.0m in height. 50 cycles/day Duty Cycle with a door speed of 14.2cm/sec. Supplied with a 24V DC 230-240 VAC 50Hz, 225W Motor and Purpose-design Gearbox. Supplied with 774ANZ Monitored Safety Beam and E960G Transmitter. Supplied with Battery Backup (Model GLD-BBU24V). Compatible with Optional Upgrade GTM-E943G-20 20 x E943G 3-Channel Visor Transmitters + 1 x E138 Wireless Wall Control. Compatible with myQ Internet Connectivity (Model G828AU separately available).