GRIFCO Model 75007 (L/R), Heavy Duty Operator for Spring Balanced Roller Shutters up to 50m² in size. Supplied with a 1.5Hp 3ph 1.10kW (2.60A) Motor and Purpose-designed Gearbox for High Cycle (30% run time) applications. Complete with Mechanical Limit System, Dust Ignition Proof Certification and Automatic Chain-Engage Mechanism (ACEM). Rated IP66. Compatible with Optional Controller Upgrade Model RG374-LB3E007-EX - Reversing Starter, Up / Stop / Down Control, Dust Ignition Proof and Mounting Plate Model MP001. Made in Australia.