GRIFCO Model 75055 (L/R), Heavy Duty Operator for Spring Balanced Roller Shutters up to 50m² in size. Supplied with a 1.5Hp 3ph 1.10kW (2.60A) Motor and Purpose-designed Gearbox for High Cycle (30% run time) applications. Complete with Mechanical Limit System and Automatic Chain-Engage Mechanism (ACEM). Rated IP55. Compatible with Optional Controller Upgrade Model RG374-LB3E007 - Reversing Starter for basic Up / Stop / Down Control and Mounting Plate Model MP001. Made in Australia.