GRIFCO Model 75065 (L/R), Heavy Duty Operator for Spring Balanced Roller Shutters up to 80m² in size. Supplied with a 2.0Hp 3ph 1.50kW (3.30A) Motor and Purpose-designed Gearbox for High Cycle (30% run time) applications. Complete with Mechanical Limit System and Automatic Chain-Engage Mechanism (ACEM). Rated IP55. Compatible with Optional Controller Upgrade Model RG374-LB3E008 - Reversing Starter for basic Up / Stop / Down Control and Mounting Plate Model MP001. Made in Australia.