GRIFCO Model 71500 (L/R), Extra Heavy Duty Operator for Spring Balanced Roller Shutters up to 100m² in size. Supplied with a 3.0Hp 3ph 2.50kW (5.70A) Motor and Purpose-designed Gearbox for High Cycle (30% run time) applications. Complete with Mechanical Limit System and 42mm Output Shaft. Rated IP50. Compatible with Optional Controller Upgrade Model RG374-LB3E009 - Reversing Starter for basic Up / Stop / Down Control and Mounting Platform Model MP003. Made in Australia.