GRIFCO Model 81500 (L/R), Extra Heavy Duty Operator for Spring Balanced Roller Shutters up to 120m² in size. Supplied with a 4.0Hp 3ph 3.00kW (5.88A) Motor and Purpose-designed Gearbox for High Cycle (30% run time) applications. Complete with Mechanical Limit System and 42mm Output Shaft. Rated IP50. Compatible with Optional Controller Upgrade Model RG374-LB3E010 - Reversing Starter for basic Up / Stop / Down Control and Mounting Platform Model MP003. Made in Australia.